# aRectifier(a,specs)

Generic analog rectifier

Function only- no corresponding object

### Syntax

o_aRectifier(a,specs)
  a: waveform - input signal
  specs: scalar record - specifications including fields:
    pol: scalar enum - polarity ("pos" or "neg")
    type: scalar enum - "full" or "half"

  return: waveform - output signal

### Usage

Simulates an ideal analog rectifier, either full or half-wave and either positive or negative polarity. Used inside various functions but can also be used directly if desired.

### Location

menu: no menu pick - to access use the Function and Object browser

library: sigLib

### Example

### Notes

### Reference

### Dependencies

### Supported On

VEE 7.0+, all platforms

### See Also

aAmp, aFilter, aMixer, aRectifier

© 2015-2017. All Rights Reserved. Stan Bischof (stan@worldbadminton.com). Last updated 20 March 2017 14:51.