(saveFormat "2.0")
(date "Tue 19/Dec/1995 09:22:13 MST")
(veerev "3.2")
(platform "HP9000s700")
(SaveCF no)
(filterNAN 0)
(component 0 ROOTCONTEXT
 (name "Taking a Reading Every Second")
 (implementation
  (retainGlobals YES)
  (locked no)
  (trigMode deg)
  (nextID 26)
  (component 0 ONCYCLE
   (interface
	(output 1
	 (name "Alarm")
	 (lock name constraints)
	)
   )
   (implementation
	(cycle 1)
   )
  )
  (component 6 BREAK
  )
  (component 7 TEXTDISPLAY
   (name "AlphaNumeric (Time Stamp Format)")
   (interface
	(input 1
	 (name "Data")
	)
   )
   (implementation
   )
  )
  (component 17 SCROLLINGTEXTDISPLAY
   (interface
	(input 1
	 (name "Data")
	)
   )
   (implementation
   )
  )
  (component 20 IFTHENELSE
   (interface
	(input 1
	 (name "A")
	 (optional yes)
	)
	(output 1
	 (name "Then")
	 (lock name constraints)
	)
	(output 2
	 (name "Else")
	 (lock name constraints)
	)
   )
   (implementation
	(expr "A>=7")
   )
  )
  (component 23 HPIDSTATE
   (name "dmm (hp34401a @ (NOT LIVE))")
   (interface
	(output 1
	 (name "READING")
	 (tag "READING")
	 (lock constraints)
	 (optional yes)
	)
   )
   (implementation
	(component filename "hp34401a.cid")
	(component driver "dmm")
	(component state
	 (idComp
	  (name "OPC_MODE")
	  (typeStr "Enum")
	  (state "Valid")
	  (value "ON")
	 )
	 (idComp
	  (name "STATUS_ENABLE")
	  (typeStr "Int16")
	  (state "Invalid")
	  (value 0)
	 )
	 (idComp
	  (name "EVENT_ENABLE")
	  (typeStr "Int16")
	  (state "Invalid")
	  (value 0)
	 )
	 (idComp
	  (name "OPER_ENABLE")
	  (typeStr "Int16")
	  (state "Invalid")
	  (value 0)
	 )
	 (idComp
	  (name "OPER_PTR")
	  (typeStr "Int16")
	  (state "Valid")
	  (value 32767)
	 )
	 (idComp
	  (name "OPER_NTR")
	  (typeStr "Int16")
	  (state "Valid")
	  (value 0)
	 )
	 (idComp
	  (name "QUESTIONABLE_ENABLE")
	  (typeStr "Int16")
	  (state "Invalid")
	  (value 0)
	 )
	 (idComp
	  (name "QUESTIONABLE_PTR")
	  (typeStr "Int16")
	  (state "Valid")
	  (value 32767)
	 )
	 (idComp
	  (name "QUESTIONABLE_NTR")
	  (typeStr "Int16")
	  (state "Valid")
	  (value 0)
	 )
	 (idComp
	  (name "BEEPSTATE")
	  (typeStr "Enum")
	  (state "Valid")
	  (value "ON")
	 )
	 (idComp
	  (name "DISPLAY_STATE")
	  (typeStr "Enum")
	  (state "Valid")
	  (value "ON")
	 )
	 (idComp
	  (name "FUNCTION")
	  (typeStr "Enum")
	  (state "Valid")
	  (value "DCV")
	 )
	 (idComp
	  (name "MATH")
	  (typeStr "Enum")
	  (state "Valid")
	  (value "OFF")
	 )
	 (idComp
	  (name "DBM_REF")
	  (typeStr "Enum")
	  (state "Valid")
	  (value "R600")
	 )
	 (idComp
	  (name "LIM_LOWER")
	  (typeStr "Real")
	  (state "Valid")
	  (value 0)
	 )
	 (idComp
	  (name "LIM_UPPER")
	  (typeStr "Real")
	  (state "Valid")
	  (value 0)
	 )
	 (idComp
	  (name "BAND_DET")
	  (typeStr "Enum")
	  (state "Valid")
	  (value "MED")
	 )
	 (idComp
	  (name "INP_IMP")
	  (typeStr "Enum")
	  (state "Valid")
	  (value "OFF")
	 )
	 (idComp
	  (name "AZERO")
	  (typeStr "Enum")
	  (state "Valid")
	  (value "ON")
	 )
	 (idComp
	  (name "MAX_TRIG")
	  (typeStr "Int16")
	  (state "Valid")
	  (value 512)
	 )
	 (idComp
	  (name "TRIG_COUNT")
	  (typeStr "Int16")
	  (state "Valid")
	  (value 1)
	 )
	 (idComp
	  (name "MAX_SAMP")
	  (typeStr "Int16")
	  (state "Valid")
	  (value 512)
	 )
	 (idComp
	  (name "SAMP_COUNT")
	  (typeStr "Int16")
	  (state "Valid")
	  (value 1)
	 )
	 (idComp
	  (name "TRIG")
	  (typeStr "Enum")
	  (state "Valid")
	  (value "IMM")
	 )
	 (idComp
	  (name "ENTRY_MODE")
	  (typeStr "Enum")
	  (state "Valid")
	  (value "FETCH_IMM")
	 )
	 (idComp
	  (name "FREQ_APER")
	  (typeStr "Enum")
	  (state "Valid")
	  (value "D5")
	 )
	 (idComp
	  (name "VOLT_APER")
	  (typeStr "Enum")
	  (state "Valid")
	  (value "D5")
	 )
	 (idComp
	  (name "FRES_APER")
	  (typeStr "Enum")
	  (state "Valid")
	  (value "D5")
	 )
	 (idComp
	  (name "CURR_APER")
	  (typeStr "Enum")
	  (state "Valid")
	  (value "D5")
	 )
	 (idComp
	  (name "DCV_AUTO")
	  (typeStr "Enum")
	  (state "Valid")
	  (value "ON")
	 )
	 (idComp
	  (name "FREQ_AUTO")
	  (typeStr "Enum")
	  (state "Valid")
	  (value "ON")
	 )
	 (idComp
	  (name "DCI_AUTO")
	  (typeStr "Enum")
	  (state "Valid")
	  (value "ON")
	 )
	 (idComp
	  (name "ACV_AUTO")
	  (typeStr "Enum")
	  (state "Valid")
	  (value "ON")
	 )
	 (idComp
	  (name "ACI_AUTO")
	  (typeStr "Enum")
	  (state "Valid")
	  (value "ON")
	 )
	 (idComp
	  (name "RES_AUTO")
	  (typeStr "Enum")
	  (state "Valid")
	  (value "ON")
	 )
	 (idComp
	  (name "DCV_RANGE")
	  (typeStr "Real")
	  (state "Invalid")
	  (value 10)
	 )
	 (idComp
	  (name "FREQ_RANGE")
	  (typeStr "Real")
	  (state "Invalid")
	  (value 10)
	 )
	 (idComp
	  (name "DCI_RANGE")
	  (typeStr "Real")
	  (state "Invalid")
	  (value 1)
	 )
	 (idComp
	  (name "ACV_RANGE")
	  (typeStr "Real")
	  (state "Invalid")
	  (value 10)
	 )
	 (idComp
	  (name "ACI_RANGE")
	  (typeStr "Real")
	  (state "Invalid")
	  (value 1)
	 )
	 (idComp
	  (name "RES_RANGE")
	  (typeStr "Real")
	  (state "Invalid")
	  (value 1000)
	 )
	 (idComp
	  (name "DELAY_AUTO")
	  (typeStr "Enum")
	  (state "Valid")
	  (value "ON")
	 )
	 (idComp
	  (name "DELAY")
	  (typeStr "Real")
	  (state "Invalid")
	  (value 0)
	 )
	 (idComp
	  (name "FAST_CONTROLLER")
	  (typeStr "Enum")
	  (state "Valid")
	  (value "NORM")
	 )
	)
   )
  )
  (component 24 NOTE
   (implementation
   )
  )
  (component 25 NOTE
   (name "Information")
   (implementation
	(text2 5
	  "This example shows how to loop an HP VEE"
	  "progrem to take an instrument reading every"
	  "second.  For further information, see"
	  "\"To Loop Part of an HP VEE Program\" in your"
	  "\"How to Use HP VEE\" manual."
	)
   )
  )
  (configuration
   (connect D4:1 D1:0)
   (connect D0:1 D2:1)
   (connect D5:1 D3:1)
   (connect D5:1 D4:1)
   (connect D0:1 D5:0)
  )
 )
 (viewFor -1
  (active detail)
  (detail
   (geometry 0 53 900 447)
   (configuration
	(viewFor 0
	 (active detail)
	 (icon
	  (iconImage "loop.icn")
	 )
	 (detail
	  (geometry 98 253 105 14)
	 )
	)
	(viewFor 6
	 (active icon)
	 (icon
	  (geometry 777 568 46 24)
	 )
	 (detail
	 )
	 (terminals on)
	)
	(viewFor 7
	 (active detail)
	 (icon
	  (geometry 0 0 247 0)
	 )
	 (detail
	  (geometry 308 229 385 22)
	  (formatter
	   (realFormat timeStamp)
	   (realSigDigits 6)
	   (realRadixSpec 4)
	   (timeStamp dateTime)
	   (timeFormat HMS H24)
	   (dateFormat WDMY)
	   (integerBase decimal)
	  )
	 )
	)
	(viewFor 17
	 (active detail)
	 (icon
	 )
	 (detail
	  (geometry 625 299 190 162)
	  (bufferSize 256)
	 )
	)
	(viewFor 20
	 (active detail)
	 (icon
	 )
	 (detail
	  (geometry 633 525 65 70)
	 )
	 (terminals on)
	)
	(viewFor 23
	 (active detail)
	 (icon
	  (geometry 0 0 222 0)
	  (iconImage "inst.icn")
	 )
	 (detail
	  (geometry 56 324 428 213)
	  (visiblePanels 8 "SET_UP" "DCV_ITEMS" "MAIN_SET" "IMPEDANCE" "AUTO_ZERO" "MULTIMETER" "MIDI_SGL" "MIDS_SIMU")
	 )
	 (terminals on)
	)
	(viewFor 24
	 (active icon)
	 (icon
	  (geometry 481 86 338 48)
	  (iconImage "disclaim.icn")
	  (label off)
	 )
	 (detail
	  (geometry 830 250 200 100)
	  (editing enabled)
	 )
	)
	(viewFor 25
	 (active detail)
	 (icon
	  (geometry 0 0 77 0)
	  (iconImage "notepad.icn")
	 )
	 (detail
	  (geometry 23 65 434 111)
	  (editing disabled)
	 )
	 (title off)
	)
	(connect D4:1 D1:0
	 (points 3 750 540 800 540 800 565)
	)
	(connect D0:1 D2:1
	 (points 4 205 260 290 260 290 240 305 240)
	)
	(connect D5:1 D3:1
	 (points 4 556 430 590 430 590 380 622 380)
	)
	(connect D5:1 D4:1
	 (points 4 556 430 580 430 580 560 600 560)
	)
	(connect D0:1 D5:0
	 (points 3 205 260 290 260 290 303)
	)
   )
   (stackingOrder 5 0 2 4 3 1 6 7)
  )
  (titleBg "Gray")
  (titleFg "Black")
  (numberFormats
   (realFormat standard)
   (realSigDigits 6)
   (realRadixSpec 4)
   (integerBase decimal)
  )
 )
)
