(saveFormat "2.3")
(date "Thu 16/Mar/2000 12:41:38 ")
(veerev "6.0 (Beta - Fokker)")
(platform "PC")
(execMode v6)
(filterNAN 0)
(workspaceStackingOrder M)
(sysconfig
(iodevice "dmm"
(type GPIB)
(gateway "This host")
(channel 7)
(subchannel 14)
(readTerm "\n")
(fs ",")
(eol "\n")
(multiField dataOnly)
(arrayFormat linear)
(timeout 5)
(byteOrder 0)
(idFileName "hp34401a.cid")
(eoiEnabled 1)
(model ""
(standard 488))))
(SaveCF no)
(device 0 ROOTCONTEXT
(properties
(trigMode deg)
(nextID 18)
(popupTitleText "Collecting Data into an Array")
(popupMoveable 1)
(popupTitleTextColor "Black")
(popupTitleBackgroundColor "Gray")
(deleteGlobals 0))
(deviceList
(device 3 FORCOUNT
(properties
(count 20))
(interface
(output 1
(name "Count")
(lock name constraints))))
(device 6 COLLECTOR
(properties
(output1D 0))
(interface
(input 1
(name "Data")
(tag "Data"))
(input 2
(type trigger)
(name "XEQ")
(lock name constraints))
(output 1
(name "Array")
(tag "Array"))))
(device 7 TEXTDISPLAY
(interface
(input 1
(name "Data"))))
(device 12 SLIDINGWINDOW
(properties
(vecSize 5)
(triggerSize 5))
(interface
(input 1
(name "Data")
(tag "Data")
(requires
(shape "Scalar"))
(lock constraints))
(output 1
(name "Array")
(tag "Array"))))
(device 13 HPIDSTATE
(properties
(name "dmm ( @ 714)"))
(interface
(output 1
(name "READING")
(tag "READING")
(optional yes)))
(implementation
(filename "hp34401a.cid")
(driver "dmm")
(state
(idComp
(name "OPC_MODE")
(typeStr "Enum")
(state "Valid")
(value "ON"))
(idComp
(name "STATUS_ENABLE")
(typeStr "Int16")
(state "Invalid")
(value 0))
(idComp
(name "EVENT_ENABLE")
(typeStr "Int16")
(state "Invalid")
(value 0))
(idComp
(name "OPER_ENABLE")
(typeStr "Int16")
(state "Invalid")
(value 0))
(idComp
(name "OPER_PTR")
(typeStr "Int16")
(state "Valid")
(value 32767))
(idComp
(name "OPER_NTR")
(typeStr "Int16")
(state "Valid")
(value 0))
(idComp
(name "QUESTIONABLE_ENABLE")
(typeStr "Int16")
(state "Invalid")
(value 0))
(idComp
(name "QUESTIONABLE_PTR")
(typeStr "Int16")
(state "Valid")
(value 32767))
(idComp
(name "QUESTIONABLE_NTR")
(typeStr "Int16")
(state "Valid")
(value 0))
(idComp
(name "BEEPSTATE")
(typeStr "Enum")
(state "Valid")
(value "ON"))
(idComp
(name "DISPLAY_STATE")
(typeStr "Enum")
(state "Valid")
(value "ON"))
(idComp
(name "FUNCTION")
(typeStr "Enum")
(state "Valid")
(value "DCV"))
(idComp
(name "MATH")
(typeStr "Enum")
(state "Valid")
(value "OFF"))
(idComp
(name "DBM_REF")
(typeStr "Enum")
(state "Valid")
(value "R600"))
(idComp
(name "LIM_LOWER")
(typeStr "Real")
(state "Valid")
(value 0))
(idComp
(name "LIM_UPPER")
(typeStr "Real")
(state "Valid")
(value 0))
(idComp
(name "BAND_DET")
(typeStr "Enum")
(state "Valid")
(value "MED"))
(idComp
(name "INP_IMP")
(typeStr "Enum")
(state "Valid")
(value "OFF"))
(idComp
(name "AZERO")
(typeStr "Enum")
(state "Valid")
(value "ON"))
(idComp
(name "MAX_TRIG")
(typeStr "Int16")
(state "Valid")
(value 512))
(idComp
(name "TRIG_COUNT")
(typeStr "Int16")
(state "Valid")
(value 1))
(idComp
(name "MAX_SAMP")
(typeStr "Int16")
(state "Valid")
(value 512))
(idComp
(name "SAMP_COUNT")
(typeStr "Int16")
(state "Valid")
(value 1))
(idComp
(name "TRIG")
(typeStr "Enum")
(state "Valid")
(value "IMM"))
(idComp
(name "ENTRY_MODE")
(typeStr "Enum")
(state "Valid")
(value "FETCH_IMM"))
(idComp
(name "FREQ_APER")
(typeStr "Enum")
(state "Valid")
(value "D5"))
(idComp
(name "VOLT_APER")
(typeStr "Enum")
(state "Valid")
(value "D5"))
(idComp
(name "FRES_APER")
(typeStr "Enum")
(state "Valid")
(value "D5"))
(idComp
(name "CURR_APER")
(typeStr "Enum")
(state "Valid")
(value "D5"))
(idComp
(name "DCV_AUTO")
(typeStr "Enum")
(state "Valid")
(value "ON"))
(idComp
(name "FREQ_AUTO")
(typeStr "Enum")
(state "Valid")
(value "ON"))
(idComp
(name "DCI_AUTO")
(typeStr "Enum")
(state "Valid")
(value "ON"))
(idComp
(name "ACV_AUTO")
(typeStr "Enum")
(state "Valid")
(value "ON"))
(idComp
(name "ACI_AUTO")
(typeStr "Enum")
(state "Valid")
(value "ON"))
(idComp
(name "RES_AUTO")
(typeStr "Enum")
(state "Valid")
(value "ON"))
(idComp
(name "DCV_RANGE")
(typeStr "Real")
(state "Invalid")
(value 10))
(idComp
(name "FREQ_RANGE")
(typeStr "Real")
(state "Invalid")
(value 10))
(idComp
(name "DCI_RANGE")
(typeStr "Real")
(state "Invalid")
(value 1))
(idComp
(name "ACV_RANGE")
(typeStr "Real")
(state "Invalid")
(value 10))
(idComp
(name "ACI_RANGE")
(typeStr "Real")
(state "Invalid")
(value 1))
(idComp
(name "RES_RANGE")
(typeStr "Real")
(state "Invalid")
(value 1000))
(idComp
(name "DELAY_AUTO")
(typeStr "Enum")
(state "Valid")
(value "ON"))
(idComp
(name "DELAY")
(typeStr "Real")
(state "Invalid")
(value 0))
(idComp
(name "FAST_CONTROLLER")
(typeStr "Enum")
(state "Valid")
(value "NORM")))))
(device 16 NOTE
(properties
(name "Information")
(text2 15 "This example shows how to use the Collector and"
"Sliding Collector objects to collect data into an"
"array. Usually, the Sliding Collector Array Size and" "Trigger are the same."
"" "1. The For Count triggers the dmm 20 times."
"2. The dmm generates a simulated reading (live mode"
"   is off) on each loop iteration."
"3. The Sliding Collector triggers after every fifth"
"   reading, outputting a one-dimensional array of" "   five readings."
"4. The Collector collects four consecutive one-"
"   dimensional arrays from the Sliding Collector,"
"   outputting all 20 readings as a two-dimensional"
"   four-by-five array to the display.")))
(device 17 NOTE
(properties
(name "Warranty Disclaimer")
(text2 4 "This example is provided as an illustration"
"\"as is\", and Agilent Technologies makes"
"no warranty of any kind with regard to this" "example.")))
(configuration
(connect D3:1 D1:1)
(connect D0:0 D1:2)
(connect D1:1 D2:1)
(connect D4:1 D3:1)
(connect D0:1 D4:0)))
(contextCarrier
(wndOrigin 2 2)
(wndState res)
(active detail)
(detail
(extent 919 525)
(anchorPt 84 131)
(configuration
(devCarrierFor 3
(active open)
(icon
(iconImage "loop.icn"))
(open
(extent 106 32))
(pinCenter 0 0))
(devCarrierFor 6
(active open)
(icon
(extent 61 25))
(open
(extent 127 67))
(terminals on)
(pinCenter 665 300))
(devCarrierFor 7
(active open)
(icon
(extent 95 24))
(open
(extent 800 124))
(pinCenter 390 460))
(devCarrierFor 12
(active open)
(icon)
(open
(extent 160 57))
(terminals on)
(pinCenter 650 180))
(devCarrierFor 13
(active open)
(icon
(extent 222 0)
(iconImage "inst.icn"))
(open
(extent 428 213)
(visiblePanels 8 "SET_UP" "DCV_ITEMS" "MAIN_SET" "IMPEDANCE" "AUTO_ZERO"
"MULTIMETER" "MIDI_SGL" "MIDS_SIMU"))
(terminals on)
(pinCenter 210 180))
(devCarrierFor 16
(active open)
(icon
(extent 77 0)
(iconImage "notepad.icn"))
(open
(extent 516 153)
(editing disabled))
(title off)
(pinCenter 550 -40))
(devCarrierFor 17
(active icon)
(icon
(extent 338 48)
(iconImage "disclaim.icn")
(label off))
(open
(extent 410 78)
(editing enabled))
(pinCenter 100 -80))
(connect D3:1 D1:1
(points 6 772 180 800 180 800 230 540 230 540 280 559 280))
(connect D0:0 D1:2
(points 5 0 18 0 30 -60 30 -60 320 559 320))
(connect D1:1 D2:1
(points 6 771 300 800 300 800 360 -30 360 -30 460 -13 460))
(connect D4:1 D3:1
(points 2 496 180 527 180))
(connect D0:1 D4:0
(points 3 55 0 230 0 230 53)))
(stackingOrder 3 0 4 1 2 5 6))
(numberFormats
(realFormat standard)
(realSigDigits 6)
(realRadixSpec 4)
(integerBase decimal))))
