(saveFormat "2.3")
(date "Thu 16/Mar/2000 12:33:08 ")
(veerev "6.0 (Beta - Fokker)")
(platform "PC")
(execMode v6)
(filterNAN 0)
(workspaceStackingOrder M)
(SaveCF no)
(device 0 ROOTCONTEXT
(properties
(trigMode deg)
(nextID 37)
(popupTitleText "Changing Values in an Array 1D")
(popupMoveable 1)
(deleteGlobals 0))
(deviceList
(device 15 FORCOUNT
(properties
(count 5))
(interface
(output 1
(name "Count")
(lock name constraints))))
(device 13 ALLOCATEARRAY
(properties
(name "Alloc Real"))
(interface
(output 1
(name "Array")
(tag "Array")))
(implementation
(numDims 1)
(dimSizes "10")
(type "Real64")
(initEnum "Init Value")
(initialValue
(data  0))
(from 1)
(thru 10)))
(device 17 NOTE
(properties
(name "Information")
(text2 20 "This example shows how to use the assignment operator"
"to change several values in a one-dimensional array." ""
"1. Alloc Real allocates a 1-dimension, ten-element array."
"2. The array of zeros is input to the JCT (Junction)"
"   object and propagates to the assignment operator."
"   The assignment operator is set up with pin A to get the"
"   array, pin B gets the array index, and pin C gets the" "   new value."
"3. The For Count repeats 5 times (0-4).  Each count sets"
"   the array index and generates a new value."
"4. When the assignment operator receives all three inputs,"
"   it outputs an array to the display and JCT with the"
"   current index on pin B set to the value on pin C."
"5. The JCT pin A receives the new array, passing it"
"   on to the assignment operator.  The cycle repeats"
"   with an incremented index from For Count, and new"
"   value from Random Number."
"6. The program ends when For Count finishes, and final"
"   values propagate to the display.")))
(device 18 FORMULA
(properties
(name "A[B] = C")
(expr 1 "A[B] = C"))
(interface
(input 1
(name "A")
(optional yes))
(input 2
(name "B")
(optional yes))
(input 3
(name "C")
(optional yes))
(output 1
(name "A")
(optional yes))))
(device 20 TEXTDISPLAY
(interface
(input 1
(name "Data"))))
(device 25 FORMULA
(properties
(name "Random Number")
(expr 1 "random(0, 1)"))
(interface
(output 1
(name "Result")
(tag "Result")
(lock name constraints)
(optional yes))))
(device 35 JUNCTION
(properties
(name "JCT"))
(interface
(input 1
(name "A"))
(input 2
(name "B"))
(output 1
(name "Data"))))
(device 36 NOTE
(properties
(name "Warranty Disclaimer")
(text2 4 "This example is provided as an illustration"
"\"as is\", and Agilent Technologies makes"
"no warranty of any kind with regard to this" "example.")))
(configuration
(connect D6:1 D3:1)
(connect D0:1 D3:2)
(connect D5:1 D3:3)
(connect D3:1 D4:1)
(connect D0:1 D5:0)
(connect D3:1 D6:1)
(connect D1:1 D6:2)))
(contextCarrier
(wndRestoredOrigin 2 2)
(wndRestoredExtent 900 447)
(wndState max)
(active detail)
(detail
(extent 911 534)
(anchorPt 805 558)
(configuration
(devCarrierFor 15
(active open)
(icon
(iconImage "loop.icn"))
(open
(extent 111 30))
(pinCenter -630 -60))
(devCarrierFor 13
(active open)
(icon)
(open
(extent 175 118))
(terminals on)
(pinCenter -565 -170))
(devCarrierFor 17
(active open)
(icon
(extent 77 0)
(iconImage "notepad.icn"))
(open
(extent 576 230)
(editing disabled))
(title off)
(pinCenter -490 -420))
(devCarrierFor 18
(active open)
(icon
(extent 57 34))
(open
(extent 86 82))
(terminals on)
(pinCenter -240 -160))
(devCarrierFor 20
(active open)
(icon)
(open
(extent 150 261))
(pinCenter -40 -90))
(devCarrierFor 25
(active icon)
(icon
(extent 116 16))
(open
(extent 107 44))
(terminals on)
(pinCenter -450 -30))
(devCarrierFor 35
(active icon)
(icon
(extent 29 25))
(open
(extent 12 50))
(terminals on)
(pinCenter -380 -200))
(devCarrierFor 36
(active icon)
(icon
(extent 338 48)
(iconImage "disclaim.icn")
(label off))
(open
(extent 410 78)
(editing enabled))
(pinCenter -20 -410))
(connect D6:1 D3:1
(points 4 -363 -200 -340 -200 -340 -180 -316 -180))
(connect D0:1 D3:2
(points 4 -572 -60 -410 -60 -410 -160 -316 -160))
(connect D5:1 D3:3
(points 4 -390 -30 -370 -30 -370 -140 -316 -140))
(connect D3:1 D4:1
(points 4 -165 -160 -140 -160 -140 -90 -118 -90))
(connect D0:1 D5:0
(points 3 -572 -60 -450 -60 -450 -41))
(connect D3:1 D6:1
(points 6 -165 -160 -140 -160 -140 -240 -410 -240 -410 -210 -397 -210))
(connect D1:1 D6:2
(points 4 -435 -170 -420 -170 -420 -190 -397 -190)))
(stackingOrder 1 4 5 0 3 6 2 7))
(numberFormats
(realFormat standard)
(realSigDigits 4)
(realRadixSpec 4)
(integerBase decimal))))
