(saveFormat "2.3")
(date "Thu 16/Mar/2000 12:30:54 ")
(veerev "6.0 (Beta - Fokker)")
(platform "PC")
(execMode v6)
(filterNAN 0)
(workspaceStackingOrder M)
(sysconfig
(iodevice "dmm"
(type GPIB)
(gateway "This host")
(channel 7)
(subchannel 14)
(readTerm "\n")
(fs ",")
(eol "\n")
(multiField dataOnly)
(arrayFormat linear)
(timeout 5)
(byteOrder 0)
(idFileName "hp34401a.cid")
(eoiEnabled 1)
(model ""
(standard 488))))
(SaveCF no)
(device 0 ROOTCONTEXT
(properties
(trigMode deg)
(nextID 27)
(popupTitleText "Taking a Reading Every Second")
(popupMoveable 1)
(popupTitleTextColor "Black")
(popupTitleBackgroundColor "Gray")
(deleteGlobals 0))
(deviceList
(device 0 ONCYCLE
(properties
(cycle 1))
(interface
(output 1
(name "Alarm")
(lock name constraints))))
(device 6 BREAK)
(device 7 TEXTDISPLAY
(properties
(name "AlphaNumeric (Time Stamp Format)"))
(interface
(input 1
(name "Data"))))
(device 17 SCROLLINGTEXTDISPLAY
(properties
(logSize 256))
(interface
(input 1
(name "Data"))))
(device 20 IFTHENELSE
(properties
(cases 1 "A>=7"))
(interface
(input 1
(name "A")
(optional yes))
(output 1
(name "Then")
(lock name constraints))
(output 2
(name "Else")
(lock name constraints))))
(device 23 HPIDSTATE
(properties
(name "dmm ( @ 714)"))
(interface
(output 1
(name "READING")
(tag "READING")
(optional yes)))
(implementation
(filename "hp34401a.cid")
(driver "dmm")
(state
(idComp
(name "OPC_MODE")
(typeStr "Enum")
(state "Valid")
(value "ON"))
(idComp
(name "STATUS_ENABLE")
(typeStr "Int16")
(state "Invalid")
(value 0))
(idComp
(name "EVENT_ENABLE")
(typeStr "Int16")
(state "Invalid")
(value 0))
(idComp
(name "OPER_ENABLE")
(typeStr "Int16")
(state "Invalid")
(value 0))
(idComp
(name "OPER_PTR")
(typeStr "Int16")
(state "Valid")
(value 32767))
(idComp
(name "OPER_NTR")
(typeStr "Int16")
(state "Valid")
(value 0))
(idComp
(name "QUESTIONABLE_ENABLE")
(typeStr "Int16")
(state "Invalid")
(value 0))
(idComp
(name "QUESTIONABLE_PTR")
(typeStr "Int16")
(state "Valid")
(value 32767))
(idComp
(name "QUESTIONABLE_NTR")
(typeStr "Int16")
(state "Valid")
(value 0))
(idComp
(name "BEEPSTATE")
(typeStr "Enum")
(state "Valid")
(value "ON"))
(idComp
(name "DISPLAY_STATE")
(typeStr "Enum")
(state "Valid")
(value "ON"))
(idComp
(name "FUNCTION")
(typeStr "Enum")
(state "Valid")
(value "DCV"))
(idComp
(name "MATH")
(typeStr "Enum")
(state "Valid")
(value "OFF"))
(idComp
(name "DBM_REF")
(typeStr "Enum")
(state "Valid")
(value "R600"))
(idComp
(name "LIM_LOWER")
(typeStr "Real")
(state "Valid")
(value 0))
(idComp
(name "LIM_UPPER")
(typeStr "Real")
(state "Valid")
(value 0))
(idComp
(name "BAND_DET")
(typeStr "Enum")
(state "Valid")
(value "MED"))
(idComp
(name "INP_IMP")
(typeStr "Enum")
(state "Valid")
(value "OFF"))
(idComp
(name "AZERO")
(typeStr "Enum")
(state "Valid")
(value "ON"))
(idComp
(name "MAX_TRIG")
(typeStr "Int16")
(state "Valid")
(value 512))
(idComp
(name "TRIG_COUNT")
(typeStr "Int16")
(state "Valid")
(value 1))
(idComp
(name "MAX_SAMP")
(typeStr "Int16")
(state "Valid")
(value 512))
(idComp
(name "SAMP_COUNT")
(typeStr "Int16")
(state "Valid")
(value 1))
(idComp
(name "TRIG")
(typeStr "Enum")
(state "Valid")
(value "IMM"))
(idComp
(name "ENTRY_MODE")
(typeStr "Enum")
(state "Valid")
(value "FETCH_IMM"))
(idComp
(name "FREQ_APER")
(typeStr "Enum")
(state "Valid")
(value "D5"))
(idComp
(name "VOLT_APER")
(typeStr "Enum")
(state "Valid")
(value "D5"))
(idComp
(name "FRES_APER")
(typeStr "Enum")
(state "Valid")
(value "D5"))
(idComp
(name "CURR_APER")
(typeStr "Enum")
(state "Valid")
(value "D5"))
(idComp
(name "DCV_AUTO")
(typeStr "Enum")
(state "Valid")
(value "ON"))
(idComp
(name "FREQ_AUTO")
(typeStr "Enum")
(state "Valid")
(value "ON"))
(idComp
(name "DCI_AUTO")
(typeStr "Enum")
(state "Valid")
(value "ON"))
(idComp
(name "ACV_AUTO")
(typeStr "Enum")
(state "Valid")
(value "ON"))
(idComp
(name "ACI_AUTO")
(typeStr "Enum")
(state "Valid")
(value "ON"))
(idComp
(name "RES_AUTO")
(typeStr "Enum")
(state "Valid")
(value "ON"))
(idComp
(name "DCV_RANGE")
(typeStr "Real")
(state "Invalid")
(value 10))
(idComp
(name "FREQ_RANGE")
(typeStr "Real")
(state "Invalid")
(value 10))
(idComp
(name "DCI_RANGE")
(typeStr "Real")
(state "Invalid")
(value 1))
(idComp
(name "ACV_RANGE")
(typeStr "Real")
(state "Invalid")
(value 10))
(idComp
(name "ACI_RANGE")
(typeStr "Real")
(state "Invalid")
(value 1))
(idComp
(name "RES_RANGE")
(typeStr "Real")
(state "Invalid")
(value 1000))
(idComp
(name "DELAY_AUTO")
(typeStr "Enum")
(state "Valid")
(value "ON"))
(idComp
(name "DELAY")
(typeStr "Real")
(state "Invalid")
(value 0))
(idComp
(name "FAST_CONTROLLER")
(typeStr "Enum")
(state "Valid")
(value "NORM")))))
(device 25 NOTE
(properties
(name "Information")
(text2 6 "This example shows how to loop an VEE"
"program to take an instrument reading every"
"second.  For further information, see the " "\"VEE Help\" topic,"
"\"To Loop Part of an VEE Program\"." "")))
(device 26 NOTE
(properties
(name "Warranty Disclaimer")
(text2 4 "This example is provided as an illustration"
"\"as is\", and Agilent Technologies makes"
"no warranty of any kind with regard to this" "example.")))
(configuration
(connect D4:1 D1:0)
(connect D0:1 D2:1)
(connect D5:1 D3:1)
(connect D5:1 D4:1)
(connect D0:1 D5:0)))
(contextCarrier
(wndOrigin 2 2)
(wndState res)
(active detail)
(detail
(extent 968 566)
(anchorPt 150 206)
(configuration
(devCarrierFor 0
(active open)
(icon
(iconImage "loop.icn"))
(open
(extent 105 14))
(pinCenter 0 0))
(devCarrierFor 6
(active icon)
(icon
(extent 46 24))
(open)
(terminals on)
(pinCenter 650 320))
(devCarrierFor 7
(active open)
(icon
(extent 247 0))
(open
(extent 385 22)
(formatter
(realFormat timeStamp)
(realSigDigits 6)
(realRadixSpec 4)
(timeStamp dateTime)
(timeFormat HMS H24)
(dateFormat WDMY)
(integerBase decimal)))
(pinCenter 350 -20))
(devCarrierFor 17
(active open)
(icon)
(open
(extent 202 159)
(noformatter))
(pinCenter 580 120))
(devCarrierFor 20
(active open)
(icon)
(open
(extent 65 70))
(terminals on)
(pinCenter 515 300))
(devCarrierFor 23
(active open)
(icon
(extent 222 0)
(iconImage "inst.icn"))
(open
(extent 428 213)
(visiblePanels 8 "SET_UP" "DCV_ITEMS" "MAIN_SET" "IMPEDANCE" "AUTO_ZERO"
"MULTIMETER" "MIDI_SGL" "MIDS_SIMU"))
(terminals on)
(pinCenter 120 170))
(devCarrierFor 25
(active open)
(icon
(extent 77 0)
(iconImage "notepad.icn"))
(open
(extent 454 126)
(editing disabled))
(title off)
(pinCenter 100 -130))
(devCarrierFor 26
(active icon)
(icon
(extent 338 48)
(iconImage "disclaim.icn")
(label off))
(open
(extent 410 78)
(editing enabled))
(pinCenter 550 -130))
(connect D4:1 D1:0
(points 3 590 280 650 280 650 305))
(connect D0:1 D2:1
(points 4 55 0 140 0 140 -20 155 -20))
(connect D5:1 D3:1
(points 4 406 170 440 170 440 120 476 120))
(connect D5:1 D4:1
(points 4 406 170 430 170 430 300 450 300))
(connect D0:1 D5:0
(points 3 55 0 140 0 140 43)))
(stackingOrder 0 2 4 1 6 5 3 7))
(numberFormats
(realFormat standard)
(realSigDigits 6)
(realRadixSpec 4)
(integerBase decimal))))
