(saveFormat "2.3")
(date "Thu 16/Mar/2000 14:37:19 ")
(veerev "6.0 (Beta - Fokker)")
(platform "PC")
(execMode v6)
(filterNAN 0)
(workspaceStackingOrder M)
(SaveCF no)
(device 0 ROOTCONTEXT
(properties
(trigMode deg)
(nextID 10)
(popupTitleText "Storing a Waveform in a File")
(popupMoveable 1)
(popupTitleTextColor "Black")
(popupTitleBackgroundColor "Gray")
(deleteGlobals 0))
(deviceList
(device 0 TOFILE
(properties
(transactions 1 "WRITE CONTAINER a"))
(interface
(input 1
(name "A")
(optional yes)))
(implementation
(attr iopath file write "wavedata"
(readTerm "\n")
(fs "\r\n")
(eol "\r\n")
(multiField fullSyntax)
(arrayFormat block))))
(device 1 FROMFILE
(properties
(transactions 1 "READ CONTAINER x"))
(interface
(output 1
(name "X")
(optional yes)))
(implementation
(attr iopath file read "wavedata"
(readTerm "\n")
(fs "\r\n")
(eol "\r\n")
(multiField fullSyntax)
(arrayFormat block))))
(device 2 VFUNCTIONGENERATOR
(properties
(function Sine)
(frequency 100)
(amplitude 1)
(dcOffset 0)
(degRad Deg)
(phaseShift 0)
(interval 0.02)
(numPoints 256))
(interface
(output 1
(name "Func")
(lock name constraints))))
(device 3 YPLOT
(properties
(name "Waveform (Time)"))
(interface
(input 1
(name "Trace1")
(lock constraints)))
(implementation
(tracePin 1)
(graphMode time)))
(device 8 NOTE
(properties
(name "Information")
(text2 4 "This example shows how to store a waveform in a"
"data file, and then retrieve that waveform."
"For further information, see the \"VEE Help\""
"topic \"To Store and Retrieve a Waveform\".")))
(device 9 NOTE
(properties
(name "Warranty Disclaimer")
(text2 4 "This example is provided as an illustration"
"\"as is\", and Agilent Technologies makes"
"no warranty of any kind with regard to this" "example.")))
(configuration
(connect D2:1 D0:1)
(connect D0:0 D1:0)
(connect D1:1 D3:1)))
(contextCarrier
(wndOrigin 2 2)
(wndState res)
(active detail)
(detail
(extent 884 559)
(anchorPt 506 229)
(configuration
(devCarrierFor 0
(active open)
(icon)
(open
(extent 235 106))
(terminals on)
(pinCenter -20 -10))
(devCarrierFor 1
(active open)
(icon)
(open
(extent 191 89))
(terminals on)
(pinCenter -160 200))
(devCarrierFor 2
(active open)
(icon
(iconImage "virtual.icn"))
(open
(extent 203 182))
(terminals on)
(pinCenter -355 10))
(devCarrierFor 3
(active open)
(icon
(iconImage "display.icn"))
(open
(extent 242 215)
(displayMode 63)
(graphType cartesian)
(gridType axis)
(scale 0
(name "Mag")
(domainName "Time")
(Yspacing 10000)
(Xspacing 10000)
(pen 9)
(show 1)
(range -1 1 4 linear))
(domain 0 0.02 4 linear)
(trace 0 onScale 0
(name "Trace1")
(pen 4)
(lineType 1)
(pointType 0)))
(pinCenter 130 200))
(devCarrierFor 8
(active open)
(icon
(extent 77 0)
(iconImage "notepad.icn"))
(open
(extent 468 99)
(editing disabled))
(title off)
(pinCenter -260 -170))
(devCarrierFor 9
(active icon)
(icon
(extent 338 48)
(iconImage "disclaim.icn")
(label off))
(open
(extent 410 78)
(editing enabled))
(pinCenter 180 -170))
(connect D2:1 D0:1
(points 4 -211 10 -190 10 -190 -10 -170 -10))
(connect D0:0 D1:0
(points 4 -20 45 -20 70 -160 70 -160 135))
(connect D1:1 D3:1
(points 2 -32 200 6 200)))
(stackingOrder 2 3 1 0 4 5))
(numberFormats
(realFormat standard)
(realSigDigits 6)
(realRadixSpec 4)
(integerBase decimal))))
