(saveFormat "2.3")
(date "Thu 26/Feb/2004 20:14:25 ")
(veerev "6.2")
(platform "PC")
(execMode v6)
(filterNAN 0)
(workspaceStackingOrder M)
(sysconfig
(iodevice "dmm"
(type GPIB)
(gateway "This host")
(channel 7)
(subchannel 22)
(readTerm "\n")
(fs ",")
(eol "\n")
(multiField dataOnly)
(arrayFormat linear)
(timeout 5)
(byteOrder 0)
(isLive 0)
(idFileName "hp34401a.cid")
(eoiEnabled 1)
(model ""
(standard 488))))
(SaveCF no)
(device 0 ROOTCONTEXT
(properties
(trigMode deg)
(nextID 15)
(popupTitleText "Storing Data for a Spreadsheet")
(popupMoveable 1)
(popupTitleTextColor "Black")
(popupTitleBackgroundColor "Gray")
(deleteGlobals 0))
(deviceList
(device 0 HPIDSTATE
(properties
(name "dmm ( @ (NOT LIVE))"))
(interface
(output 1
(name "READING")
(tag "READING")
(optional yes)))
(implementation
(filename "hp34401a.cid")
(driver "dmm")
(state
(idComp
(name "OPC_MODE")
(typeStr "Enum")
(state "Valid")
(value "ON"))
(idComp
(name "STATUS_ENABLE")
(typeStr "Int16")
(state "Invalid")
(value 0))
(idComp
(name "EVENT_ENABLE")
(typeStr "Int16")
(state "Invalid")
(value 0))
(idComp
(name "OPER_ENABLE")
(typeStr "Int16")
(state "Invalid")
(value 0))
(idComp
(name "OPER_PTR")
(typeStr "Int16")
(state "Valid")
(value 32767))
(idComp
(name "OPER_NTR")
(typeStr "Int16")
(state "Valid")
(value 0))
(idComp
(name "QUESTIONABLE_ENABLE")
(typeStr "Int16")
(state "Invalid")
(value 0))
(idComp
(name "QUESTIONABLE_PTR")
(typeStr "Int16")
(state "Valid")
(value 32767))
(idComp
(name "QUESTIONABLE_NTR")
(typeStr "Int16")
(state "Valid")
(value 0))
(idComp
(name "BEEPSTATE")
(typeStr "Enum")
(state "Valid")
(value "ON"))
(idComp
(name "DISPLAY_STATE")
(typeStr "Enum")
(state "Valid")
(value "ON"))
(idComp
(name "FUNCTION")
(typeStr "Enum")
(state "Valid")
(value "DCV"))
(idComp
(name "MATH")
(typeStr "Enum")
(state "Valid")
(value "OFF"))
(idComp
(name "DBM_REF")
(typeStr "Enum")
(state "Valid")
(value "R600"))
(idComp
(name "LIM_LOWER")
(typeStr "Real")
(state "Valid")
(value 0))
(idComp
(name "LIM_UPPER")
(typeStr "Real")
(state "Valid")
(value 0))
(idComp
(name "BAND_DET")
(typeStr "Enum")
(state "Valid")
(value "MED"))
(idComp
(name "INP_IMP")
(typeStr "Enum")
(state "Valid")
(value "OFF"))
(idComp
(name "AZERO")
(typeStr "Enum")
(state "Valid")
(value "ON"))
(idComp
(name "MAX_TRIG")
(typeStr "Int16")
(state "Valid")
(value 512))
(idComp
(name "TRIG_COUNT")
(typeStr "Int16")
(state "Valid")
(value 1))
(idComp
(name "MAX_SAMP")
(typeStr "Int16")
(state "Valid")
(value 512))
(idComp
(name "SAMP_COUNT")
(typeStr "Int16")
(state "Valid")
(value 1))
(idComp
(name "TRIG")
(typeStr "Enum")
(state "Valid")
(value "IMM"))
(idComp
(name "ENTRY_MODE")
(typeStr "Enum")
(state "Valid")
(value "FETCH_IMM"))
(idComp
(name "FREQ_APER")
(typeStr "Enum")
(state "Valid")
(value "D5"))
(idComp
(name "VOLT_APER")
(typeStr "Enum")
(state "Valid")
(value "D5"))
(idComp
(name "FRES_APER")
(typeStr "Enum")
(state "Valid")
(value "D5"))
(idComp
(name "CURR_APER")
(typeStr "Enum")
(state "Valid")
(value "D5"))
(idComp
(name "DCV_AUTO")
(typeStr "Enum")
(state "Valid")
(value "ON"))
(idComp
(name "FREQ_AUTO")
(typeStr "Enum")
(state "Valid")
(value "ON"))
(idComp
(name "DCI_AUTO")
(typeStr "Enum")
(state "Valid")
(value "ON"))
(idComp
(name "ACV_AUTO")
(typeStr "Enum")
(state "Valid")
(value "ON"))
(idComp
(name "ACI_AUTO")
(typeStr "Enum")
(state "Valid")
(value "ON"))
(idComp
(name "RES_AUTO")
(typeStr "Enum")
(state "Valid")
(value "ON"))
(idComp
(name "DCV_RANGE")
(typeStr "Real")
(state "Invalid")
(value 10))
(idComp
(name "FREQ_RANGE")
(typeStr "Real")
(state "Invalid")
(value 10))
(idComp
(name "DCI_RANGE")
(typeStr "Real")
(state "Invalid")
(value 1))
(idComp
(name "ACV_RANGE")
(typeStr "Real")
(state "Invalid")
(value 10))
(idComp
(name "ACI_RANGE")
(typeStr "Real")
(state "Invalid")
(value 1))
(idComp
(name "RES_RANGE")
(typeStr "Real")
(state "Invalid")
(value 1000))
(idComp
(name "DELAY_AUTO")
(typeStr "Enum")
(state "Valid")
(value "ON"))
(idComp
(name "DELAY")
(typeStr "Real")
(state "Invalid")
(value 0))
(idComp
(name "FAST_CONTROLLER")
(typeStr "Enum")
(state "Valid")
(value "NORM")))))
(device 1 FORCOUNT
(properties
(count 10))
(interface
(output 1
(name "Count")
(lock name constraints))))
(device 2 DELAY
(properties
(delay 3))
(interface
(output 1
(name "Done")
(tag "Done"))))
(device 3 COUNTER
(interface
(input 1
(name "Data"))
(output 1
(name "Count")
(tag "Count")
(lock name constraints))))
(device 4 TORECORD
(properties
(outputType scalar))
(interface
(input 1
(name "Cnt")
(optional yes))
(input 2
(name "Tm")
(optional yes))
(input 3
(name "Vlts")
(optional yes))
(output 1
(name "Record")
(tag "Record"))))
(device 5 FORMULA
(properties
(name "now( )")
(expr 1 "now()"))
(interface
(output 1
(name "Result")
(tag "Result")
(lock name constraints)
(optional yes))))
(device 6 TOSTRING
(properties
(transactions 1 "WRITE TEXT a TIME:HMS:H24 EOL"))
(interface
(input 1
(name "A")
(optional yes))
(output 1
(name "result")
(lock name constraints)))
(implementation
(attr iopath string write "string"
(readTerm "\n")
(fs " ")
(eol "\n")
(multiField fullSyntax)
(arrayFormat block))))
(device 9 TOFILE
(properties
(transactions 1 "WRITE TEXT a.Cnt, \" \", a.Tm, \" \", a.Vlts EOL"))
(interface
(input 1
(name "A")
(optional yes)))
(implementation
(attr iopath file write "myFile"
(readTerm "\n")
(fs "\r\n")
(eol "\r\n")
(multiField fullSyntax)
(arrayFormat block))))
(device 11 NOTE
(properties
(name "Information")
(text2 5 "This example shows how to store data in a format"
"that the Microsoft Excel spreadsheet program can"
"read.  For further information, see the" "\"VEE Help\" topic,"
"\"To Store Data for a Spreadsheet Program\".")))
(device 12 NOTE
(properties
(name "Warranty Disclaimer")
(text2 4 "This example is provided as an illustration"
"\"as is\", and Agilent Technologies makes"
"no warranty of any kind with regard to this" "example.")))
(configuration
(connect D2:1 D0:0)
(connect D1:1 D2:0)
(connect D2:1 D3:1)
(connect D3:1 D4:1)
(connect D6:1 D4:2)
(connect D0:1 D4:3)
(connect D2:1 D5:0)
(connect D5:1 D6:1)
(connect D4:1 D7:1)))
(contextCarrier
(wndOrigin 6 5)
(wndState res)
(active detail)
(detail
(extent 992 600)
(anchorPt 278 485)
(configuration
(devCarrierFor 0
(active open)
(icon
(extent 130 51)
(iconImage "inst.icn"))
(open
(extent 427 220)
(visiblePanels 8 "SET_UP" "DCV_ITEMS" "MAIN_SET" "IMPEDANCE" "AUTO_ZERO"
"MULTIMETER" "MIDI_SGL" "MIDS_SIMU"))
(terminals on)
(pinCenter -20 -20))
(devCarrierFor 1
(active open)
(icon
(iconImage "loop.icn"))
(open
(extent 110 33))
(pinCenter -210 -320))
(devCarrierFor 2
(active open)
(icon)
(open
(extent 79 35))
(pinCenter -140 -250))
(devCarrierFor 3
(active open)
(icon)
(open
(extent 105 37))
(pinCenter 0 -320))
(devCarrierFor 4
(active open)
(icon
(iconImage "build.icn"))
(open
(extent 113 91))
(terminals on)
(pinCenter 210 -240))
(devCarrierFor 5
(active icon)
(icon
(extent 48 25))
(open
(extent 69 32))
(terminals on)
(pinCenter -40 -240))
(devCarrierFor 6
(active icon)
(icon
(extent 70 25))
(open
(extent 254 78))
(terminals on)
(pinCenter 50 -240))
(devCarrierFor 9
(active open)
(icon)
(open
(extent 334 113))
(terminals on)
(pinCenter 550 -240))
(devCarrierFor 11
(active open)
(icon
(extent 77 0)
(iconImage "notepad.icn"))
(open
(extent 475 118)
(editing disabled))
(title off)
(pinCenter 370 -420))
(devCarrierFor 12
(active icon)
(icon
(extent 338 48)
(iconImage "disclaim.icn")
(label off))
(open
(extent 410 78)
(editing enabled))
(pinCenter -80 -440))
(connect D2:1 D0:0
(points 5 -98 -250 -80 -250 -80 -200 0 -200 0 -151))
(connect D1:1 D2:0
(points 3 -153 -320 -140 -320 -140 -288))
(connect D2:1 D3:1
(points 4 -98 -250 -80 -250 -80 -320 -55 -320))
(connect D3:1 D4:1
(points 4 55 -320 80 -320 80 -270 111 -270))
(connect D6:1 D4:2
(points 2 87 -240 111 -240))
(connect D0:1 D4:3
(points 4 266 -20 90 -20 90 -210 111 -210))
(connect D2:1 D5:0
(points 5 -98 -250 -80 -250 -80 -270 -40 -270 -40 -255))
(connect D5:1 D6:1
(points 2 -14 -240 12 -240))
(connect D4:1 D7:1
(points 2 329 -240 350 -240)))
(stackingOrder 2 1 6 5 7 4 8 9 3 0))
(numberFormats
(realFormat standard)
(realSigDigits 6)
(realRadixSpec 4)
(integerBase decimal))))
