(saveFormat "2.3")
(date "Thu 26/Feb/2004 20:13:54 ")
(veerev "6.2")
(platform "PC")
(execMode v6)
(filterNAN 0)
(workspaceStackingOrder M)
(sysconfig
(iodevice "HP 3852A"
(type GPIB)
(gateway "This host")
(channel 7)
(subchannel 14)
(readTerm "\n")
(fs ",")
(eol "\n")
(multiField dataOnly)
(arrayFormat linear)
(timeout 5)
(byteOrder 0)
(eoiEnabled 1)
(model ""
(standard 488))))
(SaveCF no)
(device 0 ROOTCONTEXT
(properties
(trigMode rad)
(nextID 12)
(popupTitleText "Downloading To Instruments")
(popupMoveable 1)
(popupTitleTextColor "Black")
(popupTitleBackgroundColor "Gray")
(deleteGlobals 0))
(deviceList
(device 0 NOTE
(properties
(name "Warranty Disclaimer")
(text2 4 "This example is provided as an"
"illustration \"as is\", and Agilent Technologies"
"makes no warranty of any kind" "with regard to this example.")))
(device 1 START25)
(device 2 IODEVICE
(properties
(name "HP 3852A ( @ 714)")
(transactions 1 "WRITE TEXT \"SCRATCH\" STR EOL"))
(implementation
(iopath "HP 3852A")))
(device 3 REPEATUNTILBREAK
(interface
(output 1
(name "Continuous")
(lock name constraints))))
(device 4 FROMFILE
(properties
(transactions 1 "READ TEXT x STR MAXFW:80"))
(interface
(output 1
(name "X")
(optional yes))
(output 2
(name "EOF")
(tag "EOF")
(lock name constraints)
(optional yes)))
(implementation
(attr iopath file read "~installDir/examples/manual/manual17.dat"
(readTerm "\n")
(fs " ")
(eol "\n")
(multiField fullSyntax)
(arrayFormat block))))
(device 5 IODEVICE
(properties
(name "HP 3852A ( @ 714)")
(transactions 1 "WRITE TEXT MySub STR EOL"))
(interface
(input 1
(name "Mysub")
(tag "A")
(optional yes)))
(implementation
(iopath "HP 3852A")))
(device 6 START25)
(device 7 IODEVICE
(properties
(name "HP 3852A ( @ 714)")
(transactions 1 "WRITE TEXT \"CALL BEEP2\" STR EOL"))
(implementation
(iopath "HP 3852A")))
(device 8 NOTE
(properties
(name "Thread #2")
(text2 1 "This thread calls the subroutine. ")))
(device 9 BREAK)
(device 10 NOTE
(properties
(name "Thread #1")
(text2 3 "This thread erases the HP 3852A\'s "
"subroutine memory and downloads the" "specified subroutine.")))
(device 11 NOTE
(properties
(name "Info About")
(text2 16 "Overview:" "This program illustrates one method for downloading"
"measurement subroutines or macros to programmable" "instruments. " ""
"Details:" "The program  uses the HP 3852A Data Acquisition "
"system as an example of an intelligent, programmable "
"instrument.  The subroutine \"BEEP2\" downloaded to "
"the HP 3852A simply sounds the HP 3852A beeper twice.  " ""
"The downloaded subroutine is created andmaintained "
"in a separate text file.  Thread #1 reads the text "
"file and downloads it to the instrument.  Thread #2 "
"calls the subroutine in the HP 3852A." "")))
(configuration
(connect D1:0 D2:0)
(connect D2:0 D3:0)
(connect D3:1 D4:0)
(connect D4:1 D5:1)
(connect D6:0 D7:0)
(connect D4:2 D9:0)))
(contextCarrier
(wndRestoredOrigin 166 2)
(wndRestoredExtent 900 447)
(wndState max)
(active detail)
(detail
(extent 974 758)
(anchorPt 204 10)
(configuration
(devCarrierFor 0
(active icon)
(icon
(extent 338 48)
(iconImage "disclaim.icn")
(label off))
(open
(extent 397 82)
(editing disabled))
(pinCenter -20 30))
(devCarrierFor 1
(active open)
(icon
(extent 42 15))
(open
(extent 69 39))
(title off)
(pinCenter -30 130))
(devCarrierFor 2
(active open)
(icon
(iconImage "io.icn"))
(open
(extent 271 43))
(terminals on)
(pinCenter -30 210))
(devCarrierFor 3
(active icon)
(icon
(extent 110 64)
(iconImage "loop.icn"))
(open)
(terminals on)
(pinCenter -30 280))
(devCarrierFor 4
(active open)
(icon
(extent 110 25))
(open
(extent 392 72))
(terminals on)
(pinCenter 45 390))
(devCarrierFor 5
(active open)
(icon
(iconImage "io.icn"))
(open
(extent 251 53))
(terminals on)
(pinCenter 500 390))
(devCarrierFor 6
(active open)
(icon
(extent 42 15))
(open
(extent 69 39))
(title off)
(pinCenter 20 480))
(devCarrierFor 7
(active open)
(icon
(extent 289 64)
(iconImage "io.icn"))
(open
(extent 325 52))
(terminals on)
(pinCenter 20 570))
(devCarrierFor 8
(active open)
(icon
(extent 110 0))
(open
(extent 337 46)
(editing disabled))
(pinCenter 420 570))
(devCarrierFor 9
(active icon)
(icon
(extent 78 25))
(open
(extent 70 30))
(terminals on)
(pinCenter 300 450))
(devCarrierFor 10
(active open)
(icon
(extent 110 0))
(open
(extent 362 73)
(editing disabled))
(pinCenter 490 290))
(devCarrierFor 11
(active open)
(icon
(extent 110 0))
(open
(extent 535 193)
(editing disabled))
(pinCenter 430 120))
(connect D1:0 D2:0
(points 2 -30 152 -30 168))
(connect D2:0 D3:0
(points 2 -30 234 -30 245))
(connect D3:1 D4:0
(points 3 27 280 50 280 50 333))
(connect D4:1 D5:1
(points 4 283 370 300 370 300 390 322 390))
(connect D6:0 D7:0
(points 2 20 502 20 523))
(connect D4:2 D9:0
(points 3 283 410 300 410 300 435)))
(stackingOrder 2 1 3 7 6 8 11 10 5 9 4 0))
(numberFormats
(realFormat standard)
(realSigDigits 4)
(realRadixSpec 4)
(integerBase decimal))))
