(saveFormat "2.3")
(date "Thu 26/Feb/2004 20:12:24 ")
(veerev "6.2")
(platform "PC")
(execMode v6)
(filterNAN 0)
(workspaceStackingOrder M)
(SaveCF no)
(device 0 ROOTCONTEXT
(properties
(trigMode deg)
(nextID 43)
(popupTitleText "Changing Values in an Array 1D")
(popupMoveable 1)
(deleteGlobals 0))
(deviceList
(device 15 FORCOUNT
(properties
(count 4))
(interface
(output 1
(name "Count")
(lock name constraints))))
(device 13 ALLOCATEARRAY
(properties
(name "Alloc Real"))
(interface
(output 1
(name "Array")
(tag "Array")))
(implementation
(numDims 2)
(dimSizes "4" "3")
(type "Real64")
(initEnum "Init Value")
(initialValue
(data  0))
(from 1)
(thru 10)))
(device 18 FORMULA
(properties
(name "A[B, C] = D")
(expr 1 "A[B, C] = D"))
(interface
(input 1
(name "A")
(optional yes))
(input 2
(name "B")
(optional yes))
(input 3
(name "C")
(optional yes))
(input 4
(name "D")
(optional yes))
(output 1
(name "A")
(optional yes))))
(device 20 TEXTDISPLAY
(interface
(input 1
(name "Data"))))
(device 25 FORMULA
(properties
(name "Random Number")
(expr 1 "random(0, 1)"))
(interface
(output 1
(name "Result")
(tag "Result")
(lock name constraints)
(optional yes))))
(device 35 FORCOUNT
(properties
(count 3))
(interface
(output 1
(name "Count")
(lock name constraints))))
(device 40 JUNCTION
(properties
(name "JCT"))
(interface
(input 1
(name "A"))
(input 2
(name "B"))
(output 1
(name "Data"))))
(device 41 NOTE
(properties
(name "Information")
(text2 21 "This example shows how to use the assignment operator"
"to change values in a two-dimensional array." ""
"1. Alloc Real allocates a 2-dimension array."
"2. The array of zeros is input to the JCT (Junction)"
"   object and propagates to the assignment operator."
"   The assignment operator is set up with pin A to get the"
"   array, pin B gets the array index for the rows, pin C"
"   gets the array index for the columns, and pin D gets" "   the new value."
"3. For each row (0-4) from the top For Count, all three"
"   columns get values from Random Number."
"4. When the assignment operator receives all four inputs,"
"   it outputs an array to the display and JCT with the"
"   current array location set to the value on pin D."
"5. The JCT pin A receives the new array, passing it"
"   on to the assignment operator.  The cycle repeats"
"   with an incremented indexes from the For Count objects,"
"   and new value from Random Number."
"6. The program ends when both For Count objects finishe,"
"   and final values propagate to the display.")))
(device 42 NOTE
(properties
(name "Warranty Disclaimer")
(text2 4 "This example is provided as an illustration"
"\"as is\", and Agilent Technologies makes"
"no warranty of any kind with regard to this" "example.")))
(configuration
(connect D6:1 D2:1)
(connect D0:1 D2:2)
(connect D5:1 D2:3)
(connect D4:1 D2:4)
(connect D2:1 D3:1)
(connect D5:1 D4:0)
(connect D0:1 D5:0)
(connect D2:1 D6:1)
(connect D1:1 D6:2)))
(contextCarrier
(wndRestoredOrigin 2 2)
(wndRestoredExtent 900 447)
(wndState max)
(active detail)
(detail
(extent 974 758)
(anchorPt 690 524)
(configuration
(devCarrierFor 15
(active open)
(icon
(iconImage "loop.icn"))
(open
(extent 111 30))
(pinCenter -600 -50))
(devCarrierFor 13
(active open)
(icon)
(open
(extent 212 142))
(terminals on)
(pinCenter -525 -180))
(devCarrierFor 18
(active open)
(icon
(extent 77 0))
(open
(extent 92 84))
(terminals on)
(pinCenter -250 -60))
(devCarrierFor 20
(active open)
(icon)
(open
(extent 303 134))
(pinCenter 30 -150))
(devCarrierFor 25
(active icon)
(icon
(extent 116 16))
(open
(extent 107 44))
(terminals on)
(pinCenter -430 50))
(devCarrierFor 35
(active open)
(icon
(iconImage "loop.icn"))
(open
(extent 111 30))
(pinCenter -520 10))
(devCarrierFor 40
(active icon)
(icon
(extent 29 25))
(open
(extent 12 50))
(terminals on)
(pinCenter -320 -190))
(devCarrierFor 41
(active open)
(icon
(extent 77 0)
(iconImage "notepad.icn"))
(open
(extent 570 221)
(editing disabled))
(title off)
(pinCenter -390 -400))
(devCarrierFor 42
(active icon)
(icon
(extent 338 48)
(iconImage "disclaim.icn")
(label off))
(open
(extent 410 78)
(editing enabled))
(pinCenter 90 -410))
(connect D6:1 D2:1
(points 6 -303 -190 -280 -190 -280 -150 -350 -150 -350 -90 -329 -90))
(connect D0:1 D2:2
(points 4 -542 -50 -520 -50 -520 -70 -329 -70))
(connect D5:1 D2:3
(points 4 -462 10 -430 10 -430 -50 -329 -50))
(connect D4:1 D2:4
(points 4 -370 50 -350 50 -350 -30 -329 -30))
(connect D2:1 D3:1
(points 4 -172 -60 -150 -60 -150 -150 -124 -150))
(connect D5:1 D4:0
(points 3 -462 10 -430 10 -430 39))
(connect D0:1 D5:0
(points 3 -542 -50 -520 -50 -520 -26))
(connect D2:1 D6:1
(points 6 -172 -60 -150 -60 -150 -220 -350 -220 -350 -200 -337 -200))
(connect D1:1 D6:2
(points 2 -377 -180 -337 -180)))
(stackingOrder 1 6 2 0 5 4 3 7 8))
(numberFormats
(realFormat standard)
(realSigDigits 4)
(realRadixSpec 4)
(integerBase decimal))))
