(saveFormat "2.3")
(date "Thu 26/Feb/2004 20:14:33 ")
(veerev "6.2")
(platform "PC")
(execMode v6)
(prefExecMode v8)
(filterNAN 0)
(workspaceStackingOrder M)
(sysconfig
(iodevice "dmm"
(type GPIB)
(gateway "This host")
(channel 7)
(subchannel 14)
(readTerm "\n")
(fs ",")
(eol "\n")
(multiField dataOnly)
(arrayFormat linear)
(timeout 5)
(byteOrder 0)
(isLive 0)
(idFileName "hp34401a.cid")
(eoiEnabled 1)
(model ""
(standard 488))))
(SaveCF no)
(device 0 ROOTCONTEXT
(properties
(trigMode deg)
(nextID 12)
(popupTitleText "Using a Component Driver")
(popupMoveable 1)
(popupTitleTextColor "Black")
(popupTitleBackgroundColor "Gray")
(deleteGlobals 0))
(deviceList
(device 1 TEXTDISPLAY
(interface
(input 1
(name "Data"))))
(device 2 FORCOUNT
(properties
(count 5))
(interface
(output 1
(name "Count")
(lock name constraints))))
(device 3 DELAY
(properties
(delay 3))
(interface
(output 1
(name "Done")
(tag "Done"))))
(device 4 COLLECTOR
(properties
(output1D 0))
(interface
(input 1
(name "Data")
(tag "Data"))
(input 2
(type trigger)
(name "XEQ")
(lock name constraints))
(output 1
(name "Array")
(tag "Array"))))
(device 6 HPIDINCR
(properties
(name "dmm ( @ (NOT LIVE))"))
(interface
(output 1
(name "READING")
(tag "READING")
(optional yes)))
(implementation
(filename "hp34401a.cid")
(driver "dmm")))
(device 8 NOTE
(properties
(name "Information")
(text2 5 "This example shows how to use a component driver"
"object to take readings from a digital multimeter."
"For further information, see the \"VEE Help\""
"topic \"To Use an Component Driver Object\"." "")))
(device 10 NOTE
(properties
(name "Warranty Disclaimer")
(text2 4 "This example is provided as an illustration"
"\"as is\", and Agilent Technologies makes"
"no warranty of any kind with regard to this" "example.")))
(configuration
(connect D3:1 D0:1)
(connect D1:1 D2:0)
(connect D4:1 D3:1)
(connect D1:0 D3:2)
(connect D2:1 D4:0)))
(contextCarrier
(wndOrigin 2 2)
(wndState res)
(active detail)
(detail
(extent 900 447)
(anchorPt 752 302)
(configuration
(devCarrierFor 1
(active open)
(icon)
(open
(extent 158 126))
(pinCenter 0 0))
(devCarrierFor 2
(active open)
(icon
(iconImage "loop.icn"))
(open
(extent 119 33))
(pinCenter -680 -140))
(devCarrierFor 3
(active open)
(icon)
(open
(extent 89 32))
(pinCenter -570 -70))
(devCarrierFor 4
(active open)
(icon
(extent 61 25))
(open
(extent 124 77))
(terminals on)
(pinCenter -235 20))
(devCarrierFor 6
(active open)
(icon
(extent 130 57)
(iconImage "io.icn"))
(open
(extent 198 30))
(terminals on)
(pinCenter -530 0))
(devCarrierFor 8
(active open)
(icon
(extent 77 0)
(iconImage "notepad.icn"))
(open
(extent 486 110)
(editing disabled))
(title off)
(pinCenter -130 -220))
(devCarrierFor 10
(active icon)
(icon
(extent 338 48)
(iconImage "disclaim.icn")
(label off))
(open
(extent 410 78)
(editing enabled))
(pinCenter -550 -240))
(connect D3:1 D0:1
(points 4 -131 20 -100 20 -100 0 -82 0))
(connect D1:1 D2:0
(points 3 -618 -140 -570 -140 -570 -107))
(connect D4:1 D3:1
(points 2 -359 0 -340 0))
(connect D1:0 D3:2
(points 3 -680 -121 -680 40 -340 40))
(connect D2:1 D4:0
(points 3 -523 -70 -510 -70 -510 -36)))
(stackingOrder 2 1 3 0 5 6 4))
(numberFormats
(realFormat standard)
(realSigDigits 6)
(realRadixSpec 4)
(integerBase decimal))))
