(saveFormat "2.3")
(date "Thu 26/Feb/2004 21:14:49 ")
(veerev "6.03")
(platform "PC")
(execMode v6)
(prefExecMode v9)
(filterNAN 0)
(workspaceStackingOrder M M.8)
(SaveCF no)
(device 0 ROOTCONTEXT
(properties
(trigMode deg)
(nextID 11)
(popupTitleText "Untitled")
(popupMoveable 1)
(deleteGlobals 0))
(deviceList
(device 1 YPLOT
(properties
(name "Waveform (Time)"))
(interface
(input 1
(name "Trace1")
(lock constraints)))
(implementation
(tracePin 1)
(graphMode time)))
(device 2 VFUNCTIONGENERATOR
(properties
(function Sine)
(frequency 100)
(amplitude 1)
(dcOffset 0)
(degRad Deg)
(phaseShift 0)
(interval 0.02)
(numPoints 256))
(interface
(input 1
(name "Frequency")
(tag "Frequency")
(requires
(datatype Real64)
(shape "Scalar"))
(lock constraints)
(optional yes)
(buffer YES))
(output 1
(name "Func")
(lock name constraints))))
(device 8 CONTEXT
(properties
(name "AddNoise")
(trigMode deg)
(nextID 2)
(popupTitleText "UserObject")
(popupMoveable 1))
(interface
(input 1
(name "A")
(optional yes))
(output 1
(type data)
(name "Result")
(lock constraints)
(optional yes)))
(deviceList
(device 0 VNOISEGENERATOR
(properties
(amplitude 0.401)
(numPoints 256)
(interval 0.02))
(interface
(output 1
(name "noise WF"))))
(device 1 FORMULA
(properties
(name "A + B")
(expr 1 "A + B"))
(interface
(input 1
(name "A")
(optional yes))
(input 2
(name "B")
(optional yes))
(output 1
(name "Result")
(tag "Result")
(lock name constraints)
(optional yes))))
(configuration
(connect D0:1 D1:2)
(connect D1:1 O1:1)))
(contextCarrier
(wndOrigin 90 383)
(wndState res)
(active detail)
(detail
(extent 343 216)
(anchorPt -1 -3)
(configuration
(devCarrierFor 0
(active icon)
(icon
(extent 100 51)
(iconImage "virtual.icn"))
(open
(extent 133 79))
(terminals on)
(pinCenter 110 130))
(devCarrierFor 1
(active icon)
(icon
(extent 32 25))
(open
(extent 71 42))
(terminals on)
(pinCenter 250 80))
(connect D0:1 D1:2
(points 4 162 130 180 130 180 90 231 90))
(connect D1:1 O1:1
(points 4 268 80 290 80 290 110 343 110)))
(stackingOrder 0 1))))
(device 9 INPUTDLG
(properties
(name "Int32 Input")
(popupTitle "Int32 Input")
(prompt "Enter Frequency:")
(initialValue "100")
(valueConstraint "1<=value AND value<=193")
(vErrorMessage "You must enter a number  between 1 and 193."))
(interface
(output 1
(name "Value")
(lock name constraints))
(output 2
(name "Cancel")
(lock name constraints)))
(implementation
(inputType "integer")))
(device 10 NOTE
(properties
(name "Warranty Disclaimer")
(text2 4 "This example is provided as an illustration"
"\"as is\", and Agilent Technologies makes"
"no warranty of any kind with regard to this" "example.")))
(configuration
(connect D2:1 D0:1)
(connect D3:1 D1:1)
(connect D1:1 D2:1)))
(contextCarrier
(wndOrigin 2 2)
(wndState res)
(active detail)
(detail
(extent 902 551)
(anchorPt -105 -122)
(configuration
(devCarrierFor 1
(active open)
(icon
(iconImage "display.icn"))
(open
(extent 317 279)
(displayMode 47)
(graphType cartesian)
(gridType axis)
(scale 0
(name "Mag")
(domainName "Time")
(Yspacing 1)
(Xspacing 2)
(pen 9)
(show 1)
(range -1 1 4 linear))
(domain 0 0.02 4 linear)
(trace 0 onScale 0
(name "Trace1")
(pen 4)
(lineType 1)
(pointType 0))
(markerPenColor 1))
(pinCenter 700 330))
(devCarrierFor 2
(active icon)
(icon
(extent 115 51)
(iconImage "virtual.icn"))
(open
(extent 186 175))
(terminals on)
(pinCenter 250 330))
(devCarrierFor 8
(active icon)
(icon
(extent 59 15))
(terminals on)
(pinCenter 380 330))
(devCarrierFor 9
(active icon)
(icon
(extent 62 25))
(open
(extent 435 107))
(terminals on)
(pinCenter 270 210))
(devCarrierFor 10
(active icon)
(icon
(extent 338 48)
(iconImage "disclaim.icn")
(label off))
(open
(extent 410 78)
(editing enabled))
(pinCenter 340 160))
(connect D2:1 D0:1
(points 2 412 330 539 330))
(connect D3:1 D1:1
(points 6 303 200 320 200 320 250 170 250 170 330 190 330))
(connect D1:1 D2:1
(points 2 310 330 348 330)))
(stackingOrder 0 2 1 3 4))
(numberFormats
(realFormat standard)
(realSigDigits 4)
(realRadixSpec 4)
(integerBase decimal))))
