# aAmp(a,specs)

Generic analog amplifier

Function only- no corresponding object

### Syntax

o_aAmp(a,specs)
  a: Waveform - input signal
  specs: scalar Record - record that sets specs for the amplifier
  3 fields: gain in dB, upperClip, lowerClip
  return: Waveform - output signal

### Usage

Drop this in to model an idealized non-linear amplifier with saturation.

### Location

menu: no menu pick - to access use the Function and Object browser

library: sigLib

### Example

### Notes

This implements a mathematically ideal saturating amplifier. Saturation is taken as a hard limit. It is normally hidden behind analogAmp, providing the needed functionality, but can also be used standalone.

### Reference

### Dependencies

### Supported On

VEE 7.0+, all platforms

### See Also

aFilter, aMixer, aRectifier

© 2015-2021. All Rights Reserved. Stan Bischof (stan@worldbadminton.com). Last updated 09 August 2021 18:15.