# negBridge

An ideal negative polarity full-wave rectifier.

### Syntax

none - object only

### Usage

To simulate a full-wave rectifier.

### Location

menu: veeos ==> Signal processing ==> Devices ==>negBridge

library: sigLib

### Example

### Notes

In a real world circuit, a full-wave rectifier is typically produced by using a transformer and a bridge configuration of 4 diodes. This effectively allows negative going signals through untouched and inverts positive-going signals so that all outputs are the same polarity. When used for power supplies or signal recovery, the full-wave rectifier is more complex than a half wave rectifier but at the same time is far more efficient since all of the signal passes through.

### Reference

### Dependencies

### Supported On

VEE 7.0+, all platforms

### See Also

dcBlock, posBridge, negRectifier, posRectifier

© 2015-2021. All Rights Reserved. Stan Bischof (stan@worldbadminton.com). Last updated 09 August 2021 18:23.