# aMixer(a,b,specs)

Generic analog mixer

Function only- no corresponding object

### Syntax

o_aMixer(a,b,specs)
  a: Waveform - input signal 1
  b: Waveform - input signal 2
  specs: scalar Record - specifies behavior
  fields: cl (conversion loss in dB), AXi (A signal isolation in dB), BXi (B signal isolation in dB)
  return: Waveform - the result of mixing the two input signals and adding in leakage.

### Usage

### Location

menu: no menu pick - to access use the Function and Object browser

library: sigLib

### Example

### Notes

This implements a mathematically ideal mixer with the addition of leakage signals. It is normally hidden behind upConvert and downConvert, providing the needed functionality, but can also be used standalone.

### Reference

### Dependencies

### Supported On

VEE 7.0+, all platforms

### See Also

aAmp, aFilter, aRectifier

© 2015-2021. All Rights Reserved. Stan Bischof (stan@worldbadminton.com). Last updated 09 August 2021 18:15.