I am using VEE5 on windows NT 4 with SP3 to control instruments via RS232 and RS422 in a pentium 300MHz MMX with 64 MB ram, SICL Version G.01.01.  I don't have a problem.

Adam Kohler                
Quality Assurance      
Queensferry Microwave Division   
Hewlett-Packard Ltd    
Station Road                 
South Queensferry
West Lothian
Scotland
EH30 9TG        

-----Original Message-----
From:	umar@mdr.indra-espacio.es [SMTP:umar@mdr.indra-espacio.es]
Sent:	Tuesday, October 06, 1998 10:59 AM
To:	hpvxd_xc@hpislsup.lvld.hp.com
Subject:	VRF: WNT4.0 and RS232

Hi folks!
We are using VEE4.01 on Windows NT 4.0 with Service Pack 3 to control an
equipment via serial line RS232 in a Pentium 166 MMX (32 MHz RAM), SICL
version is F.0101. Our application is OK for minutes and then it doesn4t
respond.

Does anybody have any experience with this?

Any help would be appreciated.
--
Ursicio Javier Martin Martino
INDRA ESPACIO (Earth Stations Department)
Mar Egeo, 4
28850 San Fernando de Henares (Madrid)
Tfno.: 913963331; E-mail: umar@mdr.indra-espacio.es