(saveFormat "2.3")
(date "Mon 20/Mar/2000 14:56:41 ")
(veerev "6.0 (Beta - Fokker+)")
(platform "PC")
(execMode v6)
(filterNAN 0)
(workspaceStackingOrder M)
(SaveCF no)
(device 0 ROOTCONTEXT
(properties
(trigMode deg)
(nextID 2)
(popupTitleText "Untitled")
(popupMoveable 1)
(deleteGlobals 0))
(deviceList
(UserFunctions
(nextID 4)
(context 0
(properties
(name "BuildRecAry")
(trigMode deg)
(nextID 6)
(popupTitleText "UserFunction1")
(popupMoveable 1))
(interface
(output 1
(type data)
(name "X")
(lock constraints)
(optional yes)))
(deviceList
(device 0 FORCOUNT
(properties
(count 4))
(interface
(output 1
(name "Count")
(lock name constraints))))
(device 1 FORMULA
(properties
(name "random(low,high)")
(expr 1 " random(0,1)"))
(interface
(output 1
(name "Result")
(tag "Result")
(lock name constraints)
(optional yes))))
(device 2 CONSTANT
(properties
(name "Int32"))
(interface
(output 1
(name "Int32")
(lock name constraints)))
(implementation
(value Int32
(data  5))
(initValue Int32
(data  0))))
(device 3 FORMULA
(properties
(expr 1 " (A<=5 ? \"PASS\" : \"FAIL\")"))
(interface
(input 1
(name "A")
(optional yes))
(output 1
(name "Result")
(tag "Result")
(lock name constraints)
(optional yes))))
(device 4 TORECORD
(properties
(outputType scalar))
(interface
(input 1
(name "Value")
(optional yes))
(input 2
(name "Limit")
(optional yes))
(input 3
(name "PassFail")
(optional yes))
(output 1
(name "Record"))))
(device 5 COLLECTOR
(properties
(output1D 0))
(interface
(input 1
(name "Data")
(tag "Data"))
(input 2
(type trigger)
(name "XEQ")
(lock name constraints))
(output 1
(name "Array")
(tag "Array"))))
(configuration
(connect D0:1 D1:0)
(connect D1:1 D3:1)
(connect D1:1 D4:1)
(connect D2:1 D4:2)
(connect D3:1 D4:3)
(connect D4:1 D5:1)
(connect D0:0 D5:2)
(connect D5:1 O1:1)))
(contextCarrier
(active detail)
(detail
(extent 793 405)
(anchorPt 1 0)
(configuration
(devCarrierFor 0
(active open)
(icon
(iconImage "loop.icn"))
(open
(extent 95 31))
(pinCenter 70 50))
(devCarrierFor 1
(active open)
(icon
(extent 106 0))
(open
(extent 128 42))
(terminals on)
(pinCenter 140 130))
(devCarrierFor 2
(active open)
(icon)
(open
(extent 67 29)
(showFormat int))
(pinCenter 230 230))
(devCarrierFor 3
(active open)
(icon)
(open
(extent 238 50))
(terminals on)
(pinCenter 250 320))
(devCarrierFor 4
(active open)
(icon
(iconImage "build.icn"))
(open
(extent 169 151))
(terminals on)
(pinCenter 500 120))
(devCarrierFor 5
(active icon)
(icon
(extent 53 25))
(open
(extent 96 54))
(terminals on)
(pinCenter 650 360))
(connect D0:1 D1:0
(points 3 120 50 150 50 150 88))
(connect D1:1 D3:1
(points 6 256 130 280 130 280 170 80 170 80 320 98 320))
(connect D1:1 D4:1
(points 4 256 130 290 130 290 70 353 70))
(connect D2:1 D4:2
(points 4 266 230 300 230 300 120 353 120))
(connect D3:1 D4:3
(points 6 421 320 440 320 440 250 330 250 330 170 353 170))
(connect D4:1 D5:1
(points 6 647 120 670 120 670 220 610 220 610 350 621 350))
(connect D0:0 D5:2
(points 5 70 68 70 80 20 80 20 370 621 370))
(connect D5:1 O1:1
(points 4 679 360 700 360 700 202 791 202)))
(stackingOrder 0 4 1 5 2 3))))
(context 1
(properties
(name "ReportBody")
(trigMode deg)
(nextID 2)
(popupTitleText "UserFunction1")
(popupMoveable 1))
(interface
(input 1
(name "A")
(optional yes)))
(deviceList
(device 0 TOFILE
(properties
(transactions 2 "WRITE TEXT A[B].Value, \"|\", A[B].Limit, \"|\" REAL64 FIX:4"
"WRITE TEXT A[B].PassFail STR FW:5 RJ EOL"))
(interface
(input 1
(name "A")
(optional yes))
(input 2
(name "B")
(optional yes)))
(implementation
(attr iopath file write "report.txt"
(readTerm "\n")
(fs "\r\n")
(eol "\r\n")
(multiField fullSyntax)
(arrayFormat block))))
(device 1 FORCOUNT
(properties
(count 3))
(interface
(output 1
(name "Count")
(lock name constraints))))
(configuration
(connect I1:1 D0:1)
(connect D1:1 D0:2)))
(contextCarrier
(active detail)
(detail
(extent 624 344)
(anchorPt 0 0)
(configuration
(devCarrierFor 0
(active open)
(icon)
(open
(extent 477 148))
(terminals on)
(pinCenter 340 120))
(devCarrierFor 1
(active open)
(icon
(iconImage "loop.icn"))
(open
(extent 95 31))
(pinCenter 110 310))
(connect I1:1 D0:1
(points 4 0 171 10 171 10 80 69 80))
(connect D1:1 D0:2
(points 6 160 310 180 310 180 250 30 250 30 160 69 160)))
(stackingOrder 1 0))))
(context 2
(properties
(name "ReportDisplay")
(trigMode deg)
(nextID 5)
(popupMoveable 1))
(deviceList
(device 0 FROMFILE
(properties
(transactions 1 "READ TEXT x STR ARRAY:*"))
(interface
(output 1
(name "X")
(optional yes)))
(implementation
(attr iopath file read "report.txt"
(readTerm "\n")
(fs "\r\n")
(eol "\r\n")
(multiField fullSyntax)
(arrayFormat block))))
(device 3 SCROLLINGTEXTDISPLAY
(properties
(logSize 256))
(interface
(input 1
(name "Data"))))
(device 4 CONFIRM25
(properties
(name "DONE"))
(interface
(output 1
(name "Go")
(lock name constraints)))
(implementation))
(configuration
(connect D0:1 D1:1)
(connect D1:0 D2:0))
(ShowOnExecPanel
(relativeOrigin 355 178)))
(contextCarrier
(active panel)
(panel
(extent 288 271)
(widget 1 detail
(relativeOrigin 10 10)
(title off)
(borderStyle flat)
(extent 257 203)
(formatter
(realFormat standard)
(realSigDigits 4)
(realRadixSpec 4)
(integerBase decimal)))
(widget 2 detail
(relativeOrigin 100 240)
(title off)
(borderStyle none)
(extent 47 22)))
(detail
(extent 648 351)
(anchorPt 0 0)
(configuration
(devCarrierFor 0
(active open)
(icon)
(open
(extent 231 108))
(terminals on)
(pinCenter 180 110))
(devCarrierFor 3
(active open)
(icon)
(open
(extent 257 203)
(formatter
(realFormat standard)
(realSigDigits 4)
(realRadixSpec 4)
(integerBase decimal)))
(title off)
(pinCenter 500 150))
(devCarrierFor 4
(active open)
(icon
(extent 39 0))
(open
(extent 47 22))
(title off)
(pinCenter 500 310))
(connect D0:1 D1:1
(points 4 328 110 350 110 350 150 369 150))
(connect D1:0 D2:0
(points 2 500 254 500 296)))
(stackingOrder 0 1 2))))
(context 3
(properties
(name "ReportHeader")
(trigMode deg)
(nextID 1)
(popupTitleText "UserFunction1")
(popupMoveable 1))
(deviceList
(device 0 TOFILE
(properties
(transactions 5 "WRITE TEXT \"LIMIT TEST\" EOL"
"WRITE TEXT \"==============\" EOL" "WRITE TEXT now() DATE:DMY TIME:HM:H12 EOL"
"WRITE TEXT \"==============\" EOL"
"WRITE TEXT \"Value     Limit      Result\" EOL"))
(implementation
(attr iopath file write "report.txt"
(readTerm "\n")
(fs "\r\n")
(eol "\r\n")
(multiField fullSyntax)
(arrayFormat block))))
(configuration))
(contextCarrier
(active detail)
(detail
(extent 488 242)
(anchorPt 0 0)
(configuration
(devCarrierFor 0
(active open)
(icon)
(open
(extent 363 157))
(terminals on)
(pinCenter 230 110)))))))
(device 0 NOTE
(properties
(text2 12 "BuildRecAry: Simulates test data and stores it in an array "
"     of records." ""
"ReportHeader: Sends a report header to the specified file   "
"     consisting of a test name, a time stamp, and table headings"
"     for three columns of test data." ""
"ReportBody: Sends a test value, test limit, and pass/fail"
"     indicator for three tests to the specified file." ""
"ReportDisplay: Displays the report from the specified file." "")))
(device 1 NOTE
(properties
(name "Warranty Disclaimer")
(text2 4 "This example is provided as an illustration"
"\"as is\", and Agilent Technologies makes"
"no warranty of any kind with regard to this" "example.")))
(configuration))
(contextCarrier
(wndOrigin 2 2)
(wndState res)
(active detail)
(detail
(extent 708 424)
(anchorPt 0 0)
(configuration
(devCarrierFor 0
(active open)
(icon
(iconImage "notepad.icn"))
(open
(extent 565 237)
(editing enabled))
(pinCenter 330 160))
(devCarrierFor 1
(active icon)
(icon
(extent 338 48)
(iconImage "disclaim.icn")
(label off))
(open
(extent 410 78)
(editing enabled))
(pinCenter 220 340)))
(stackingOrder 0 1))
(numberFormats
(realFormat standard)
(realSigDigits 4)
(realRadixSpec 4)
(integerBase decimal))))
